EUFD Preset tuning

Press Preset button; looks like a P under the brightness knob
RTS rocker to select radio to tune
WCA Rocker to select freq from preset list on the right. 
Press Enter key to tune your radio


Tuning UHF/VHF radios using MPD

M button, R6 COM 
	This is where you edit your presets for the EUFD PRESET Menu; there are 10 preset channels.
Click B2, MAN
Tune either VHF or UHF radios from left row; T2 and T3 are GUARD freqs and are permanent(?)
	Enter frequency on CDU, press Enter
		Should see your entered freq under the radio you just changed on the MPD.
The above listed works for every radio on the left menu. Currently there is no way to 
edit the preset name, coming later in EA. 

To manually tune a VHF frequency via the COM page, perform the following:
1. COM fixed action button – Press.
2. MAN (B2) – Select.
3. VHF FREQ> (L1) – Select and enter frequency with the KU.

To manually tune a UHF frequency via the COM page, perform the following:
1. COM fixed action button – Press.
2. MAN (B2) – Select.
3. UHF FREQ> (L2) – Select, and enter frequency with the KU.

To manually tune an FM frequency via the COM page, perform the following:
1. COM fixed action button – Press.
2. MAN (B2) – Select.
3. FM1 FREQ> (L3) – Select, and enter frequency with the KU, or
3. FM2 FREQ> (L4) – Select, and enter frequency with the KU.

To manually tune an HF frequency via the COM page, perform the following:
1. COM fixed action button – Press.
2. MAN (B2) – Select
3. HF RECV FREQ> (R1) – Select, and enter frequency with the KU.
4. HF RECV EMISSION (R2) – Select and set appropriately.
5. HF XMIT FREQ> (R3) – Select, and enter frequency with the KU.
6. HF XMIT EMISSION (R4) – Select and set appropriately.