Input waypoint
	Select TSD bottom row
	- B6 Point
	- PB L2 ADD
		--WayPoint, HaZard, ControlMeasures, TarGet
	- PB L1 IDENT ^^
		CDU pops up IDENT, apply 2 digit ABR; IE LZ for landing zone, ect
		FREE pops up, enter 3 digit anything to help memorize like ICAO code
		UTM Lat/Long pop up - enter this in either MGRS or Lat/LONG format
			first 5 digits should be autofilled if using MGRS..if not, you will have to convert
			to lat/long
		Alt pops up, press enter or correct
	-Repeat for next waypoints 

Create the route
	-PB B5 RTE
	-PB L5 DIR
		-Select WP01 on left side
	the first waypoint will activate the rest in order of entering upon entering Wp1 as direct.

To create waypoints via cursor
	-Point
	-TG, CM etc... ADD
	- slew cursor to desired point on map and depress
	
To connect flight plan
	-RTE
	-Add, slew cursor over to desired first wpt
	-Press END on r/h side
	-Slew cursor over to desired next wpt
	-Press END; first part of the route will be displayed as a line from 1 to 2
	-Continue with wp3 and so forth

To delete a point
	-Point
	-Select wpt to delete
	-delete Y/N

You can go direct to any waypoint by pressing DIR, then slewing your cursor to the wpt you wish to fly to.
