waypoint 1
left MFD bottom row - point (highlight)
keft MFD left row - Add (highlight)
left MFD select what applies: HZ, CM, WP, TG
	HZ = hazards such as terrain, or waypoints - 01-50
	CM = control measures - friendlies or enemy units or airfields - 51-99
	WP = waypoint
	TG = Target 1-50
left MFD top left row - Ident
	top row, select ABR for appropriate abbreviation of waypoint identity - lz for landing zone
CDU - Ident will display; type in LZ (or approp abbrev), press enter
	free displays - enter your 3 letter description at will or just press enter
	UTM LAT/LON: by default current a/c location is given on left upper MFD, press enter for 
		wp 1
	 altitude - press enter 

wpt 2
	in the F10 map, press Lalt Y to cycle grid type to get proper coordinates
New coordinates to be entered into CDU but only Lat/Long decimals. You can use the CDU for basic math
to convert coordinates from decimal seconds to seconds - ie 34.90\60

left MFD bottom row - point (highlight)
keft MFD left row - Add (highlight)
left MFD top left row - Ident 
CDU - Ident will display; (select appropriate abbrev, this case AE for enemy armor), select enter. 
	CM should have been selected automatically since AE was used for ident
	Free Text - PRI (primary), enter, then enter your coordinates in either MGRS or LatLong.
		To be able to show this waypoint (enemy armor), upper row, SHOW highlight, select COORD
		SHOW, then left side select all you want applied to show.

wpt 3 onwards, you can use a cursor from wp2 to create next waypoint
	select Left Bottom - POINT, left row ADD, WP, use cursor and depress where you want it

to display the route you created - press RTE bottom row, slew cursor over waypoints in any order, cursor enter to select. Press End on the right to add to end the sequence and do so for each waypoint in order. 
Target points cant be added to the route, so a waypoint close to the target area should be selected in a tactically. 

To create the route, select Add, cursor slew to waypoint (current aircraft position first), press end. Slew to next wpt and repeat until route is drawn. To delete a wpt, select DEL, press the designated wpt to delete on the right or select with cursor, select YES or NO. 

