TADS FLIR/TV - map to joystick, LHG
LHG compensation button (LHC)  - - - - - - causes issues on MP atm so only SP for now
LHG Store/Update switch - lase target, then hit this button to store target in memory

TADS - Day/Night
Boresite IHADDS
Arm LASER
	Wep/Util/Laser

ACQ - set as desired -
	PHD (pilot head), GHS (gunner head), TAD, SKR (other ship), FCR or FXD

Store targets - B1 button - PHASE ATK highlighted, will show up under coordinates T5 button
listed as waypoints
	on the MAP page when you lase, the target will be highlighted by a cross with a line from own ship
	successful store will show up as a red T* on the map
To bring the stored target into view, select ACQ HMD, COORD, target you wish to slave to, press SLAVE.
Press slave again to slew the sensor for fine adjustments.

Armament - Arm
TEDAC - pick sensor of interest RHG
	Slew sensor around using TAD, or use HMD
	

Proper set up for hellfires before launch
	WAS Hellfire
	CHAN - Pick a channel from up top and select laser code (ex CH1, A 1688) on left, return to weps page
	CODE - pick the code you just selected for your channel above (1688)
		A-F are preset laser codes for the weps system; L-R  are for the rangefinder
	Verify LRFD matches PRI (LRFD A, PRI A)
	Check missile status; should list Pri channel (A) and (R) for ready if lasing yourself

	If all parameters are good, ok for launch