getting started :

LRFD  -  Laser Rangefinder Designator
LST - Laser Spot Track

Armament A/S - arm
weapons page - LST and LRFD - deconflict codes first. 
	Code (highlight) - select an option from left menu for laser codes
		manually, go to FREQ
		check CDU - * FREQ (being selection, ie B), enter your laser code, enter. You can also use it 			as a scratch pad - type in 4 numbers, then select which code you wish to enter it in on 				the left side left MFD, then hit enter on CDU.
ACQ -TADS

Pri (*A) PRF 
ALT (B) PIM - - these are channels; Select Chan top row (1-4)

Right side MFD (SAL = Semi Active Laser, RF = Radar)
Mode - Norm, RIPL, MAN = deals with how the aircraft selects the next missile to shoot
Traj - Low, Hi, Dir =  DIR is TADS or HMD LOS. LO is low popup, HI is high popup. 
LRFD - determines what part of the laser the missile will target- foreground laser scatter or background


target area

ACQ source TADS slaved to IHADS - monocle should go from FLIR to overlay showing bright spots as targets.
	Pick a target, deslave and fine tune from the TADS. 
Weapon Action Switch RIGHT - missile

Check TADS for LRFD weapon handoff type - REMOTE - assumes someone is lasing for you.
	To right of ARM checkerboard, LRFD A = change appropriate. Change PRI back to ALPHA 
		Left side Left MFD - PRI - select A, remote message s/b gone
TYP - SAL
MODE - NORM
TRAJ - DIR

Arm, LASE by pressing second stage trigger, reticle should cross out, TADS should display *range
	you can choose to store target in memory should you need to at this point by selecting Store Update
	on left hand grip on the TADS. Will list as T-00* on the TSD map. you can get the info from the COORD 	page and relay info. Select as ACQ source to swing the TADS back onto target. 

1. (CPG) Sight select – TADS.
2. (CPG) Weapon – Weapon Action Switch (WAS) – Right to MSL.
3. Arm/Safe button – ARM (Performed by crewmember not on the controls).
4. (CPG) Range – Set as desired or verify in the HAD Range/Range Source field.
5. (CPG) Messages – Verify no inhibits are displayed. Verify trajectory and mode is displayed as desired in HAD Weapon Status field.
6. (Optional, if launching LOBL) Designate – Squeeze TEDAC RHG laser trigger, 2nd detent.
7. (Optional, if launching LOBL) Messages (CPG) – Verify no inhibits are displayed. Verify “PRI CHAN TRK” is displayed in the HAD Weapon Status field if launching LOBL.

	Lase immediately or delayed lase. Lase first to store in memory, set as ACQ source